Prodew Install Checklist

1. Upon Arrival
   * Verify Water Supply
   * Verify Drain
   * Verify Electrical Supply
   * Picture of existing department
   * Locate equipment Shipped
2. Open boxes and inspect Equipment
   * Verify All parts were sent
3. Inspect Installation location
   * Picture of current case
   * Determine where holes need to be drilled for tracks
4. Install System
   * Caulk all new holes drilled for installation
   * Caulk and existing Unused Holes
5. After Insulation
   * Complete Work order
6. If you were instructed to do something different than instructed
   * Notify Supervisor
   * Verify the instructor is a manager and has authorization to make the change
   * Have manager sign off on the change
   * Take pictures of instructed change
7. After Installation Pictures/video’s Required
   * Video of system operating
   * Entire department
   * Entire Case - Front
   * Entire Case - Top
   * Entire Case - Sides
   * Entire Case - Back
   * Misting Tracks
   * Misting Box
   * Timer Box
   * Timer Settings
   * Control Box Gauge while running
   * Compressor
   * Compressor Pressure Gauge While running
   * RO System
   * Holes Drilled through case (Caulked)
   * Water Hookup
   * Electrical Hookup
   * Drain Line (secured)
   * All water connections
8. Send all pictures and work order in after completion