Prodew Install Checklist

1. Upon Arrival
	* Verify Water Supply
	* Verify Drain
	* Verify Electrical Supply
	* Picture of existing department
	* Locate equipment Shipped
2. Open boxes and inspect Equipment
	* Verify All parts were sent
3. Inspect Installation location
	* Picture of current case
	* Determine where holes need to be drilled for tracks
4. Install System
	* Caulk all new holes drilled for installation
	* Caulk and existing Unused Holes
5. After Insulation
	* Complete Work order
6. If you were instructed to do something different than instructed
	* Notify Supervisor
	* Verify the instructor is a manager and has authorization to make the change
	* Have manager sign off on the change
	* Take pictures of instructed change
7. After Installation Pictures/video’s Required
	* Video of system operating
	* Entire department
	* Entire Case - Front
	* Entire Case - Top
	* Entire Case - Sides
	* Entire Case - Back
	* Misting Tracks
	* Misting Box
	* Timer Box
	* Timer Settings
	* Control Box Gauge while running
	* Compressor
	* Compressor Pressure Gauge While running
	* RO System
	* Holes Drilled through case (Caulked)
	* Water Hookup
	* Electrical Hookup
	* Drain Line (secured)
	* All water connections
8. Send all pictures and work order in after completion